Front Bumper Modification

	
	Cooling measure that 1 
" 5/6 type ち っ く air intakes " 
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* Consideration 
As for the FD from 5 types the derived wind to the air cleaner became modification. 
From while derived wind guiding who inhalation is done until recently in the one for intercooler the air chamber 
By way of, to the air cleaner the derived wind having done, from 5 types the intercooler 
To become independent system completely, from the license plate reverse side the air chamber passing 
To the air cleaner it reached the point where the derived wind it does. 
As for merit of this system ardor inside engine compartment core of intercooler passing 
It means that it was gone that it flows into to air cleaner side. 
When (temperature of the incoming air goes down 4 degrees, output 3 horsepower) rises by the car of 1% (300ps) 

Usually, this is actualized with the FD of the time before 4 types, the bumper of 5/6 types is necessary, but 
If it processes, the similar effect it can obtain even with the old type bumper. 

In addition, being to know, you make at the rough sketch look, it does, but the intake of 5/6 types has been attached on the number reverse side. 
This position being to be good does, while travelling but the モワッ it is emitted from while and ラジエター side parking 
It is in the position where the hot blast is sucked. 
You think at this point in time the method of having introduced with the coconut, can inhale the air whose temperature is lower. 
At the time of especially travelling, inertia it is supercharged. (The effect saying to there!) 
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* Necessary thing 
- Courage (the hole is bored through the bumper being * & *) 
- Drill and hole saw 
- Paper for finish 
- Driver 
- In order the bumper primer (close adhesion of the paint to improve) 
- The paint (with the colour other than brilliant black, whether the bonnet part and the like and colour is not agreeable, * & *) 
If (the eye which was seen is not designated as the air, colour it is not necessary to paint, as it is, but * & *) 
- Clearing (applying the final coating) 
- Duct 
- The stay for the license plate (1 type does not need, don't you think? is) 
- Because is, in order the net (the eye which was seen to improve, option) 
* Operation 1 
First the front bumper is removed. 
Method of removing please refers to this way. 

When you can remove, you bore the hole of size how much with some kind of カタチ 
While looking at the actually bumper, you think. 
The one which is larger than the license plate as for the effect is higher, but the hole is visible from before. 
In addition, after 2 types the genuine license plate stay is stopped with the rivet being 
Considering the position of that hole, it is necessary to position. 
(Try to crush the hole) 

When shape and size are decided, the oily pen and the ダーマトグラフ (the alias デルマ) with the marking it does. 
Accurately in order to become centre, please note. 

The hole is bored prudently with the drill and the hole saw and the hot knife et cetera. 
Opening to the small awakening, while the paper (the sandpaper) with arranging shape, fine was adjusted the one which it is finished cleanly, probably will be. 

Shape is arranged with the paper. 600th 800th please finish finally with. 
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The person whom it does not paint may advance to the next, is, but as for the person who is painted doing the foot attaching, the bumper primer painting, it paints. If (the eye which was seen is seriously considered, the coconut degree of hardness is highest!) As for the part which you can remove removing entirely, after the masking doing any which you cannot remove cleanly, it paints. When it paints, having become the citron skin, surely " it is owner-occupied home paint! " With it is the feeling which is said, because you think, the paper (2000th) you apply, the buff apply with the compound. 
(Those where it becomes the citron skin with for the general can spray are helpless thing) 

* Operation 2 
The hole is bored through also the reinforcement next. 
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Like the circle the figure yellow " the hole of the bumper compared to the hole is bored through just a little large texture ". 
Because the reinforcement is made making use of the glass fiber, 
When you work with the bare hand, it does prickly. 
This several weeks you do not take prickly. 
By any means if well, doing, please work e.g., the rubber glove is set. 
Because the material of the reinforcement is not hard so, with the drill metallurgy saw 
It can process simply. 

Installing the bumper lastly as before, installing the duct inside, it is completion. 

* In duct being attached 
Because the duct to inside adhere you can adhere even with time saddle, just a little you write. 
Even with when the duct is not attached, you think the air flows into with just the ち ょ っ into the engine compartment, being 
Being not to be it does, that " boring the hole there is no meaning ", but 
After all, therefore with special care, the derived wind it does to the air cleaner. 

It seems that is introduced in the magazine but (you did not know), the genuine air chamber of 5 types 
Don't you think? it seems that is also the method of using. 
Because the hole opens the chamber of 5 types in the downward look, just the duct to over there it should have made, we would like to see, is. 
Simply, that hole is being not to be circle the duct (usually circle) with problem of connection and, 
When it orders 5 type chambers, 6280 Yen it does. 
As for me being to think it is wasted, the genuine part made the duct with the method of not using. 
By the way, if it orders this part, " fresh air duct item turn N3G1-13-201 " is. 
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This 
Before making the duct, as for we want remembering as extra knowledge, " from when idling always 
Vacuum occurs, (the air is inhaled)" with means saying. 
When the air is vacuum, because " the one which is easy to inhale (the one whose resistance is little) from there is a character which inhales ", 
In order not to inhale ardor, the place where we do not want inhaling (close) with accurately the opening of the heat source closing, 
Way the duct that tries does not become unnecessarily long, even the maximum supercharging time in the air quantity a room is 
There is a necessity such that of thickness of the duct is thought. 

As for the material of the air duct, those of the aluminum for the air conditioning which is sold well are general. 
You can buy even at the car supply store, but because it is high unjustly, is bought with foam/home center and the HANDS et cetera the one which 
It is attached cheaply. 
I have not been attached like the photograph attaching rectilinear, with the photograph still, but 
It closed the entrance of the air cleaner BOX and the opening of the duct with the thick adhesion tape. 
When here opens, inhaling ardor, because the stripe you thought uninformed, is. 
If this aluminum duct 2 it is, even at when opening fully as for the air quantity you think whether it is not all right. 
(As for truth after 1 we would like to attach) 
In addition, because this part the opening of the bonnet is very narrow, with 1 as for the duct of thick type 
It is not possible to pass. 
It hits against the bonnet. 
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Don't you think? (the point of the duct is visible. As for the flow of the air becoming rectilinear, you think as the る.) 
When the duct is installed, like the photograph please close the hole which is opened in the duct of the intercooler. 

If you adhere, it can make more real duct, for example (because FRP formation and the like) with you think, 
The person who adheres please tries persevering. 


Head Light Modification

Air intake (outlet?) Processing 
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* Consideration 
Always holding thermal problem, it increases the FD. 
Normally riding, just is fixed to just a little procrastination, water temperature is not inquiring normal to the To roller which 
It rises. 
As for being effective to cooling, 

* Front bumper spoiler exchange (enlargement of opening) 
* Rear of the bonnet is increased, (the effect is high, but design deteriorates) 
* Aero the bonnet (the effect is high, but when the rain enters, price is expensive) 
* In the ラジエター whose coefficient of thermal conductivity is high exchange (as for being fixed turn, 5 types (the 280ps) the genuine ラジエター) 
* Chilled water チューン (billion thermo- no cod * & * and so on. As for the ホド of the effect it is not understood) 
* The FAN two tries to turn cooling the ファンチューン (not turning the air conditioner to a ON) 

And so on is known well. 
There being a money, if still the roof being attached parking zone, the aero bonnet is good, probably will be. 
It has gone here, as for " air intake processing " as for the effect it is thinner than above-mentioned every one, is. 
Clearly speaking * & * 
Change is born to so and 1st to be cheap, because the eye which was seen, cost performance is high, is. 

* Process method 
First, either headlight cover (the lamp lid) you bore the hole, it decides. 
Because only the commodity " of the right side " it has come out the tuning shop of any, 
The right side most being settled in the purpose which you saw, it probably is to be visible. 
Because the turbine (the heat source) there is a right side, there is also a reason which is said, probably will be. 
Of course, being both, you are not concerned. 
As for the eye which you saw? Is, but. 

When the one which you remove is decided, first it is disassembly. 
First the light/write is opened, this cover is removed. 
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Please do not turn the screw other than 4 in the figure. 
Because it is the screw for optical axis adjustment, when it turns, the optical axis slips. 
Because it is in a state where top is caught to the cover with the nail, while to try to push in the downward look, when it pulls, it comes off. 

The headlight cover is removed next. 
It has remained with volt/bolt 4. (Before 2, rear 2) 
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First closing the retractor bull light/write, you remove 2 of rear, open the light/write and the person who removes anterior 2 is good, probably will be. 
If only volt/bolt it loosens, the husband れ it increases simply. 

Well, first, " the drill ". 
Don't you think? just a little courage it needs. 
So, failing, for if you buy the part " 4530 Yen ", you can reset to the origin. 

You bore the hole " of some カタチ " " of which extent " " somewhere, or " decide. 
When it is decided, being really to bore the hole, it does, but I opened with the soldering iron. 
The iron the knife has been attached first, if the " hot knife ", you think furthermore it is simple. 
There is also a method of boring the many holes with the drill, keeping connecting the hole, but time is required. 
When the hole is bored with each method, with the cutting blade which the リューター and the drill is attached first, it keeps arranging the カタチ of the hole. 
End arranges the カタチ with the waterproof paper. 
The slope it could point me gently, (photograph reference) 

Simply, if only the hole opens, being to be awkward (it is possible to be that! With as for the one which is said please throw), 
The net which it is possible with the aluminum is stuck from reverse side. 
It is possible to glue with whatever, is, but the method which chooses those which are difficult to receive the influence of heat is more appealing. 
By the way, it can purchase " the net " with foam/home center and Tokyu Hands. They are not high ones. 

Until it dries, it waits. 

Well, next " the foot you attach and " are. 
" The foot to attach ", with, before the painting doing the water grinding with the 600th from 1000th about paper, 
It is the job which the coating film that tries does not peel off by designating the surface finely as the ギザギザ. 
This time the partner to be soft with the plastic, in addition also the paint being to use " software 99 ", (this way reference) 
The 1000th water we have decided to grind with. 
While pouring the water, please grind the surface which it paints evenly. 
After if grinding, it tries not to touch by the hand, it can also exclude the time of removal of fat. 

When grinding it ends, the moisture is made to dry completely. 
Especially because the part " of the アミ " does not dry forever, please use the dryer. 
When (you bring close too much, it dissolves and the ち ゃ is!) 

" The masking " it is next. 
This time basically as for the masking there is no necessity, just the person that, but " as for the net we would like to put out the taste of the aluminum ", 
The masking it does in the net part. 

Blowing the surfacer, painting, you blow clear. 
It is not necessary, as for the surfacer to be, is, but. 
Because you grind afterwards, clear blows many times fully. 

Whole day and night it makes dry. 
When it is possible, the オススメ it does that 3 days or more it makes dry completely. 

1000th beginning from, the water you grind with the 2000th up to waterproof paper. 
If it soaks uniformly with the water, somewhere has done the still convex concavity, it is the expectation which is visible. 
Concave there is no convex, at the same time, layer of body color under polishes does not appear. 
Lastly, the next day being prepared that myalgra it becomes, enhances with the compound. 
2000th you ground with, if is, it is the expectation where gloss comes out directly. 
If the polisher of electromotion or the air - it is, however it is easy, don't you think? * & * 

* Supplementation 
The person who has self-confidence in modelling with the putty making the form of the complete intake protrude probably is possible. 
The rain entering from here, because the light/write is gets wet, that much as for problem you think it is not. 
Installation of the headlight cover, in order Chile (the opening of the body, the difference in level) to be agreeable, opens many times, closing doing 
After fine adjusting, please " tighten securely ". 
Unless here it is agreeable, " accident car kana? " With it is thought. 
Then, this part 
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If you remove, furthermore as for cooling efficiency you think it rises. But (as for the rain you think it becomes easy to enter) 

