	EManage Connector
	Pin Number
	Wire Colour
	Orig ECU signal
	Pin Number

	
	
	
	
	

	Ignition Input Signal CH6
	1 (A)
	LB/W
	
	

	Ignition Input Signal CH5
	2 (A)
	P/W
	
	

	Ignition Input Signal CH4
	3 (A)
	PL/W
	
	

	Ignition Input Signal CH2
	4 (A)
	O/W
	tL
	1H

	Ignition Input Signal CH1
	5 (A)
	L/W
	tT
	1G

	Ignition Output Signal CH6
	6 (A)
	LB/B
	
	

	Ignition Output Signal CH5
	7 (A)
	P/B
	
	

	Ignition Output Signal CH4
	8 (A)
	PL/B
	
	

	Ignition Output Signal CH3
	9 (A)
	Y/B
	
	

	Ignition Input Signal CH3
	10 (A)
	Y/W
	
	

	Ignition Output Signal CH2
	11 (A)
	O/B
	Leading Coil
	

	Ignition Output Signal CH1
	12 (A)
	L/B
	Trailing Coil
	

	
	
	
	
	

	Airflow (F) / VTEC Input
	13 (B)
	LB
	BAC Valve Duty
	3Q

	Airflow2 (V) In / VTEC out
	14 (B)
	Y
	Water Injection Pump
	

	Airflow1 (V) Input
	15 (B)
	W
	From Air Meter
	

	TPS Input
	16 (B)
	GY
	TPS Full Range
	2G

	Injector Input Signal CH1
	17 (B)
	L/R
	Front Primary
	3W

	Injector Input Signal CH2
	18 (B)
	O/R
	Rear Primary
	3Y

	Injector Input Signal CH3
	19 (B)
	Y/R
	Front Secondary
	3X

	Injector Input Signal CH4
	20 (B)
	PL/R
	Rear Secondary
	3Z

	Airflow (F) Input
	21 (B)
	PL
	
	

	Airflow1 (V) Output
	22 (B)
	G
	Airflow Meter
	2B

	RPM Signal Input
	23 (B)
	BR
	Ignition Leading
	1H

	Ground (ECU)
	24 (B)
	B
	Ground
	3A,3B,3C

	Ignition Power
	25 (B)
	R
	+B
	1B

	Injector Input Signal CH7
	26 (B)
	W/R
	Intake Temp Warn rly
	

	Injector Input Signal CH8
	27 (B)
	G/R
	RAD Fan B/UP Relay
	

	Injector Input Signal CH5
	28 (B)
	P/R
	Water Inj Solenoid
	

	Injector Input Signal CH6
	29 (B)
	LB/R
	Water Spray Relay
	 (NVCS)

	Injector/Sensor Ground
	30 (B)
	B/R
	Analog Ground
	3D

	
	  
	
	
	

	Analog Voltage Input
	31 (C)
	W/G
	From MAP Sensor
	

	Knock 1 /Water Temp
	32 (C)
	L/Y
	Water Thermo
	2E

	Crank Angle Signal Input
	33 (C)
	GY/W
	Crank Angle (Ne)
	3E

	Injector Output Signal CH1
	34 (C)
	L/GY
	Front Primary Injector
	

	Injector Output Signal CH2
	35 (C)
	O/GY
	Rear Primary Injector
	

	Injector Output Signal CH3
	36 (C)
	Y/GY
	Front Secondary Inj
	

	Analog Voltage Output
	37 (C)
	G/GY
	Pressure Sensor
	2H

	Knock 2  /Intake Temp
	38 (C)
	PL/Y
	Engine Intake temp
	2L

	Cam Angle Signal Input
	39 (C)
	GY/B
	Crank Angle (G)
	3G

	Vehicle Speed Signal Out
	40 (C)
	BR/Y
	
	

	Vehicle Speed Signal In
	41 (C)
	LB/Y
	From Cruise Control
	

	Injector Output Signal CH4
	42 (C)
	PL/GY
	Rear Secondary Inj
	

	Injector Output Signal CH5
	43 (C)
	P/GY
	
	

	Injector Output Signal CH6
	44 (C)
	LB/GY
	
	

	
	
	
	
	


