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look at the bottom pic, that’s all the locations of the main bolts and are 14mm for side ones by gear stick and the rest 10mm.

you will need to remove the vent covers from the sides and also the  one on top of the dash. Remove the gearstick assy.

The pic does not show the two 14mm bolts that go either side of the steering wheel of which you will need to remove the steering plastic cowling top and bottom to get at them.

The electrics there are x3 plugs by fuse box and one you will get at once you have pulled it apart a bit which is in the top of the dash behind the idiots display.
